# “Andromeda” Console Implementation Notes

Kjell has created a new PCB for the ANDROMEDA front panel prototype. This has a lot more encoders and pushbuttons, and uses an MCP23017 to interface 16 buttons via I2C.

# Control Layout

# 

Figure 2: Initial V2 Prototype (for test only)



Figure : V3 Prototype

## Encoder Functions:

From a software perspective, each dual encoder can have A (upper) and B (lower) encoders plus a “click” function. s/w numbering allows up to 20 numbers making encoders 1-40 and switches 1-20

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Encoder**  **Schematic numbers** | **Prototype V3** | | | **Early Prototype V2** | | |
| **Function** | **Encoder report #** | **Switch**  **s/w#** | **Function** | **Encoder report #** | **Switch**  **s/w#** |
| (2A) | RX1 AF | 1 |  | RX1 AF | 1 |  |
| (2B) | RX1 AGC | 2 |  | RX1 AGC | 2 |  |
| 2 click | RX1 mute |  | 1 | RX1 mute |  | 1 |
| 3A | Filter high | 3 |  | Filter high | 3 |  |
| 3B | Filter low | 4 |  | Filter low | 4 |  |
| 3 Click | Filter reset |  | 3 | Filter reset |  | 3 |
| 4A | Div’ty gain | 5 |  | Div’ty gain | 5 |  |
| 4B | Div’ty phase | 6 |  | Div’ty phase | 6 |  |
| 4 Click | Fast/slow |  | 5 | Fast/slow |  | 6 |
| 5A | Multifunction | 7 |  | Mic gain | 7 |  |
| 5B | N/A | 8 |  | Drive | 8 |  |
| 5 Click | Multi |  | 7 | (none) |  | 7 |
| 6A | RX2 AF | 9 |  | RX2 AF | 9 |  |
| 6B | RX2 AGC | 10 |  | RX2 AGC | 10 |  |
| 6 Click | RX2 mute |  | 9 | RX2 mute |  | 9 |
| 7A | RIT | 11 |  | Compander | 11 |  |
| 7B | N/A | 12 |  | Master AF | 12 |  |
| 7 Click | RIT/XIT step |  | 11 | Comp on/off |  | 11 |
| 8A | N/A |  |  | Multifunction | 13 |  |
| 8B | N/A |  |  | Squelch | 14 |  |
| 8 Click | N/A |  |  | Multi |  | 13 |

(note encoder switch numbers have been done so that encoder report number 13 corresponds to switch 13. If it is a dual encoder that also has encoder 14 on the same footprint, 14 can’t have a switch)

## Pushbutton Functions

(encoders start at 1; pushbuttons start at 21)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Pushbutton report number | Prototype V3 | | | Prototype V2 | | |
| s/w scan code | CPU pin | function | s/w scan code | CPU pin | function |
| 1 | 6 | DIG6 | Encoder 1 click | 6 | DIG6 | Encoder 1 click |
| 3 | 17 | DIG53 | Encoder 2 click | 17 | DIG53 | Encoder 2 click |
| 5 | 8 | DIG23 | Encoder 3 click | 8 | DIG23 | Encoder 3 click |
| 7 | 9 | DIG29 | Encoder 4 click | 9 | DIG29 | Encoder 4 click |
| 9 | 27 | DIG61 | Encoder 5 click | 25 | DIG61 | Encoder 5 click |
| 11 | 0 | DIG50 | Encoder 6 click | 26 | DIG62 | Encoder 6 click |
| 13 | - | - | No encoder | 27 | DIG63 | Encoder 7 click |
| 21 | 1 | ANA3 | F1 | 1 | ANA3 | F1 |
| 22 | 2 | ANA4 | F2 | 2 | ANA4 | F2 |
| 23 | 3 | ANA5 | F3 | 3 | ANA5 | F3 |
| 24 | 4 | ANA6 | F4 | 4 | ANA6 | F4 |
| 25 | 5 | ANA7 | F5 | 5 | ANA7 | F5 |
| 26 | 7 | DIG9 | F6 / NR | 30 | DIG66 | PS ON/F6 |
| 27 | 16 | DIG52 | F7 / NB | 31 | DIG67 | SINGLE CAL/F8 |
| 28 | 35 | DIG69 | F8 / SNB | 32 | DIG68 | 2 TONE/F7 |
| 29 | 10 | DIG40 | RIT+ | 0 | ANA2 | RIT- |
| 30 | 11 | DIG41 | BAND- | 7 | DIG9 | NR |
| 31 | 12 | DIG42 | MODE- | 10 | DIG40 | RIT+ |
| 32 | 13 | DIG43 | SDR ON | 11 | DIG41 | BAND- |
| 33 | 14 | DIG44 | BAND+ | 12 | DIG42 | MODE- |
| 34 | 15 | DIG45 | MODE+ | 13 | DIG43 | SDR ON |
| 35 | 18 | ANA6 | FILTER- | 14 | DIG44 | BAND+ |
| 36 | 19 | ANA5 | FILTER+ | 15 | DIG45 | MODE+ |
| 37 | 20 | DIG54 | RIT ON | 16 | DIG52 | NB |
| 38 | 21 | DIG55 | A/B TOGGLE | 18 | DIG54 | RIT ON |
| 39 | 22 | DIG56 | MOX | 19 | DIG55 | A/B TOGGLE |
| 40 | 23 | DIG57 | TUNE | 20 | DIG56 | MOX |
| 41 | 24 | DIG58 | CLICK TUNE | 21 | DIG57 | TUNE |
| 42 | 25 | DIG59 | VFO LOCK | 22 | DIG58 | CLICK TUNE |
| 43 | 26 | DIG60 | A > B | 23 | DIG59 | VFO LOCK |
| 44 | 28 | DIG62 | VFO SYNC | 24 | DIG60 | A > B |
| 45 | 29 | DIG63 | RIT- | 28 | DIG64 | SPLIT |
| 46 | 30 | DIG64 | SPLIT | 29 | DIG65 | B > A |
| 47 | 31 | DIG65 | B > A | 33 | DIG69 | SNB |
| 48 | 32 | DIG66 | PS ON |  |  |  |
| 49 | 34 | DIG68 | 2 TONE TEST |  |  |  |

(DIG67, scan code 33, is unused)

(encoder numbers correspond to the 1st encoder number. So encoder 3,4 has switch scan code 3)

## Indicator Functions

(starting at 1)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Indicator report number | Prototype V3 | | Prototype V2 | |
| s/w number | function | s/w number | function |
| 1 | 0 | VFO Lock on | 0 | VFO Lock on |
| 2 | 1 | Puresignal on | 1 | Puresignal on |
| 3 | 2 | MOX | 2 | MOX |
| 4 | 3 | Tune 1 | 3 | Tune 1 |
| 5 | 4 | Click Tune On | 4 | Click Tune On |
| 6 | 5 | VFO Sync On | 5 | COMP On |
| 7 | 6 | NB On | 6 | SQL On |
| 8 | 7 | RIT On | 7 | RIT On |
| 9 | 8 | Tune 2 | 8 | Tune 2 |
| 10 | 9 | NR On | No LED |  |
| 11 | 10 | SNB On | No LED |  |
| 12 | 11 | XIT On | No LED |  |

# Arduino Software Structure

## Concept for Operation

The front panel controller will exchange simple messages with the SDR application (eg Thetis) so that all the “radio” functionality is in one place, to minimise latency. The controller will debounce buttons and encoders and pass the results for processing.

The serial queue to / from the PC will use normal Arduino library code. Simple TX commands will be generated for each pushbutton or encoder event. RX commands will be processed for indicator setting, to allow s/w version to be queried and potentially to allow encoder rates to be adjusted.

## Serial Command Set

This should be quite simple. CAT compatible commands proposed.

|  |  |  |
| --- | --- | --- |
| **Control type** | **Command** | **Meaning** |
| VFO encoder | Up: ZZZUnn;  Down: ZZZDnn; | nn = number of clicks (0-99) |
| Other encoder | ZZZEnnm; | nn = encoder number:  0: unused  1-20: encoder 1-20, clockwise  51-70: encoder 1-20, anticlockwise  m=number of clicks (0-9) |
| Pushbutton (including encoder) | ZZZPnnm; | nn=button number (1-99, 0=n/a);  m=0: released; m=1: pressed; m=2: long pressed (not supported yet) |
| Indicator | ZZZInnm; | nn=indicator number (1-99, 0=n/a);  m=0: unlit; m=1: lit |
| Query hardware version | ZZZH;  Response ZZZHmm; | mm=0: V2 (early prototype);  mm=1: V3 (current prototype) |
| Query s/w Version | ZZZS;  Response ZZZSmmm; | mmm= s/w version |

After serial connection established, the unit will send a hardware version report “ZZZHmm;”

# Arduino Libraries

Arduino Due has the Atmel SAM3X8E ARM Cortex-M3 processor. Any input can have an interrupt and it may be possible to select the h/w input debounce. But needs some specific libraries

* “DueFlashStorage” library is an EEPROM equivalent library for Due
* Timer – Due specific “DueTimer”
* Serial – there seem to be several. “Serial” is the normal one. “SerialUSB” is the “native” port not used in this application.

# Rotary Encoders

Interrupt driven code is poor at debouncing. It does work well with bounce-free optical encoders.

Zacsketches/quadrature works well for the VFO: I’m getting 2400 steps per revolution.

ClickEncoder works well for the other “mechanical” encoders.

# Arduino Hardware



## I2C ports

I2C port 1 (DIG20, DIG21) connect to MCP23017. Chip address = 0x20. Class: Wire

I2C port 2 (SCL1, SDA1) connect to J10 for TX2 interface (note no pullup resistors) Class: Wire1

## CPU Pin Assignments – 2nd Prototype

#define V3HARDWARE

Encoder inputs and LEDs are all connected to Arduino pins. Note that the analogue pins can be assigned digital functions too.

15 pushbuttons are connected to an MCP23017; 20 are directly connected to the Arduino (total=35). The Encoder pushbuttons currently end up with the last s/w numbers, because the EncoderHandleButton function (encoders.c) just subtracts the 1st encoder button number to find which encoder it is assigned to. But that could be done a different way eg with a lookup table.

New hardware pin IDs:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Pin Name** | **Function** | **Connector** | **Pin Name** | **Function** | **Connector** |
| Digital 0 / RX0 | Reserved USB | PWML | Digital 31 | LED10 | Digital |
| Digital 1/ TX0 | Reserved USB | PWML | Digital 32 | LED4 | Digital |
| Digital 2 | VFO encoder | PWML | Digital 33 | LED5 | Digital |
| Digital 3 | VFO encoder | PWML | Digital 34 | LED6 | Digital |
| Digital 4 | Encoder 2A | PWML | Digital 35 | SW63 | Digital |
| Digital 5 | Encoder 2A | PWML | Digital 36 | LED13 | Digital |
| Digital 6 | Enc 2 SW | PWML | Digital 37 | LED7 | Digital |
| Digital 7 | Encoder 2B | PWML | Digital 38 | LED8 | Digital |
| Digital 8 | Encoder 2B | PWMH | Digital 39 | Encoder 6B | Digital |
| Digital 9 | SW17 | PWMH | Digital 40 | SW11 | Digital |
| Digital 10 | Encoder 3A | PWMH | Digital 41 | SW12 | Digital |
| Digital 11 | Encoder 3A | PWMH | Digital 42 | SW13 | Digital |
| Digital 12 | Encoder 6B | PWMH | Digital 43 | SW14 | Digital |
| Digital 13 LED | Reserved LED | PWMH | Digital 44 | SW15 | Digital |
| Digital 14 TX3 | Encoder 3B | communication | Digital 45 | SW16 | Digital |
| Digital 15 RX3 | Encoder 3B | Communication | Digital 46 | Encoder 6A | Digital |
| Digital 16 TX2 | SW58 | Communication | Digital 47 | Encoder 6A | Digital |
| Digital 17 RX2 | Encoder 4A | Communication | Digital 48 | Encoder 7A | Digital |
| Digital 18 TX1 | LED12 | Communication | Digital 49 | Encoder 7A | Digital |
| Digital 19 RX1 | (Unused) | Communication | Digital 50 | ENC 7 SW | Digital |
| Digital 20 SDA | Reserved SDA | Communication | Digital 51 | LED11 | Digital |
| Digital 21 SCL | Reserved SCL | Communication | Digital 52 | SW18 | Digital |
| Digital 22 | Encoder 4A | Digital | Digital 53 | Enc3 SW | Digital |
| Digital 23 | Enc4 SW | Digital | Analog 0 | LED2 | Analog In |
| Digital 24 | Encoder 4B | Digital | Analog 1 | LED3 | Analog In |
| Digital 25 | Encoder 4B | Digital | Analog 2 | (unused) | Analog In |
| Digital 26 | SW59 | Digital | Analog 3 | SW46 | Analog In |
| Digital 27 | Encoder 5A | Digital | Analog 4 | (unused) | Analog In |
| Digital 28 | Encoder 5A | Digital | Analog 5 | SW48 | Analog In |
| Digital 29 | Enc5 SW | Digital | Analog 6 | SW49 | Analog In |
| Digital 30 | LED1 | Digital | Analog 7 | SW50 | Analog In |
| Digital 54 | SW9 | MCP23017 | Digital 62 | SW56 | MCP23017 |
| Digital 55 | SW1 | MCP23017 | Digital 63 | SW10 | MCP23017 |
| Digital 56 | SW2 | MCP23017 | Digital 64 | SW8 | MCP23017 |
| Digital 57 | SW3 | MCP23017 | Digital 65 | SW7 | MCP23017 |
| Digital 58 | SW4 | MCP23017 | Digital 66 | SW21 | MCP23017 |
| Digital 59 | SW5 | MCP23017 | Digital 67 | (unused) | MCP23017 |
| Digital 60 | SW6 | MCP23017 | Digital 68 | SW20 | MCP23017 |
| Digital 61 | Enc6 SW | MCP23017 | Digital 69 | SW22 | MCP23017 |

10 mechanical Encoders (4 dual, 2 single) + VFO:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Kjell number** | **A function** | **B function** | **s/w number** | **Enc A pin** | **Enc B pin** |
| 2 | RX1 AF gain | RX1 RF gain | 0, 1 | DIG4, DIG5 | DIG7, DIG8 |
| 3 | Filter High cut | Filter Low cut | 2, 3 | DIG10, DIG11 | DIG14, DIG15 |
| 4 | Diversity gain | Diversity phase | 4, 5 | DIG17, DIG22 | DIG24, DIG25 |
| 6 | RX2 AF gain | RX2 RF gain | 6, 7 | DIG46, DIG47 | DIG12, DIG39 |
| 5 | Multifunction | ---- | 8 | DIG27, DIG28 | ---- |
| 7 | RIT | ---- | 9 | DIG48, DIG49 | ---- |

29 s/w connected pushbuttons + 6 encoder press; 0-19 direct, 20-35 via MCP32017 (in blue):

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Kjell SW number** | **s/w** | **Function** | **pin** | **Kjell SW number** | **s/w** | **Function** | **pin** |
| SW1 | 21 | A/B toggle | DIG55 | SW56 | 28 | VFO SYNC | DIG62 |
| SW2 | 22 | MOX | DIG56 | SW20 | 34 | 2 TONE TEST | DIG68 |
| SW3 | 23 | TUNE | DIG57 | SW21 | 32 | PURESIGNAL ON | DIG66 |
| SW4 | 24 | Click TUNE | DIG58 | SW22 | 35 | F8 key / SNB | DIG69 |
| SW5 | 25 | VFO LOCK | DIG59 | SW58 | 1 | F1 key | ANA3 |
| SW6 | 26 | A > B | DIG60 | SW59 | 2 | F2 key | ANA4 |
| SW7 | 31 | B > A | DIG65 | SW63 | 3 | F3 key | ANA5 |
| SW8 | 30 | SPLIT | DIG64 | SW50 | 4 | F4 key | ANA6 |
| SW9 | 20 | RIT ON | DIG54 | SW46 | 5 | F5 key | ANA7 |
| SW10 | 29 | RIT - | DIG63 | ENC2 SW | 6 | RX1 MUTE | DIG6 |
| SW11 | 10 | RIT + | DIG40 | ENC3 SW | 17 | FILTER RESET | DIG53 |
| SW12 | 11 | BAND - | DIG41 | ENC4 SW | 8 | DIVERSITY FINE/COARSE | DIG23 |
| SW13 | 12 | MODE - | DIG42 | ENC5 SW | 9 | Multifunction | DIG29 |
| SW14 | 13 | SDR ON | DIG43 | ENC6 SW | 27 | RX2 MUTE | DIG61 |
| SW15 | 14 | BAND + | DIG44 | ENC7 SW | 0 | RIT/XIT toggle | DIG50 |
| SW16 | 15 | MODE + | DIG45 | SW49 | 18 | FILTER- | ANA6 |
| SW17 | 7 | F6 key / NR | DIG9 | SW48 | 19 | FILTER+ | ANA5 |
| SW18 | 16 | F7 key / NB | DIG52 | SW23 |  | Power (not via Arduino) | N/A |

(DIG67, S/w 33, unused)

12 s/w connected LEDs (note LED9 is directly powered by Vdd, not s/w):

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Kjell LED number** | **s/w number** | **Function** | **Pin** | **Comment** |
| LED1 | 5 | VFO SYNC | DIG30 |  |
| LED2 | 6 | NB | ANA0 |  |
| LED3 | 2 | MOX | ANA1 |  |
| LED4 | 3 | TUNE on | DIG32 |  |
| LED5 | 4 | CTUNE on | DIG33 |  |
| LED6 | 0 | LOCK on | DIG34 |  |
| LED7 | 1 | PS on | DIG37 |  |
| LED8 | 7 | RIT on | DIG38 |  |
| LED10 | 8 | TUNE on | DIG31 | ATU ready for Andromeda |
| LED11 | 9 | NR | DIG51 |  |
| LED12 | 10 | SNB | DIG18 |  |
| LED13 | 11 | XIT | DIG36 |  |

## CPU Pin Assignments – 1st Prototype

#define V2HARDWARE

Encoder inputs and LEDs are all connected to Arduino pins. Note that the analogue pins can be assigned digital functions too.

16 pushbuttons are connected to an MCP23017; 18 are directly connected to the Arduino (total=34). The Encoder pushbuttons currently end up with the last s/w numbers, because the EncoderHandleButton function (encoders.c) just subtracts the 1st encoder button number to find which encoder it is assigned to. But that could be done a different way eg with a lookup table.

Remember the Ext MOX input with Odin hardware presents itself as an extra button; we don’t have one with V2 hardware.

New hardware pin IDs:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Pin Name** | **Function** | **Connector** | **Pin Name** | **Function** | **Connector** |
| Digital 0 / RX0 | Reserved USB | PWML | Digital 31 | LED10 | Digital |
| Digital 1/ TX0 | Reserved USB | PWML | Digital 32 | LED4 | Digital |
| Digital 2 | VFO encoder | PWML | Digital 33 | LED5 | Digital |
| Digital 3 | VFO encoder | PWML | Digital 34 | LED6 | Digital |
| Digital 4 | Encoder 2A | PWML | Digital 35 | Encoder 8B | Digital |
| Digital 5 | Encoder 2A | PWML | Digital 36 | Encoder 8B | Digital |
| Digital 6 | Enc 2 SW | PWML | Digital 37 | LED7 | Digital |
| Digital 7 | Encoder 2B | PWML | Digital 38 | LED8 | Digital |
| Digital 8 | Encoder 2B | PWMH | Digital 39 | Encoder 6B | Digital |
| Digital 9 | SW17 | PWMH | Digital 40 | SW11 | Digital |
| Digital 10 | Encoder 3A | PWMH | Digital 41 | SW12 | Digital |
| Digital 11 | Encoder 3A | PWMH | Digital 42 | SW13 | Digital |
| Digital 12 | Encoder 6B | PWMH | Digital 43 | SW14 | Digital |
| Digital 13 LED | Reserved LED | PWMH | Digital 44 | SW15 | Digital |
| Digital 14 TX3 | Encoder 3B | communication | Digital 45 | SW16 | Digital |
| Digital 15 RX3 | Encoder 3B | Communication | Digital 46 | Encoder 6A | Digital |
| Digital 16 TX2 | Encoder 5B | Communication | Digital 47 | Encoder 6A | Digital |
| Digital 17 RX2 | Encoder 4A | Communication | Digital 48 | Encoder 7A | Digital |
| Digital 18 TX1 | Encoder 7B | Communication | Digital 49 | Encoder 7A | Digital |
| Digital 19 RX1 | Encoder 7B | Communication | Digital 50 | Encoder 8A | Digital |
| Digital 20 SDA | Reserved SDA | Communication | Digital 51 | Encoder 8A | Digital |
| Digital 21 SCL | Reserved SCL | Communication | Digital 52 | SW18 | Digital |
| Digital 22 | Encoder 4A | Digital | Digital 53 | Enc3 SW | Digital |
| Digital 23 | Enc4 SW | Digital | Analog 0 | LED2 | Analog In |
| Digital 24 | Encoder 4B | Digital | Analog 1 | LED3 | Analog In |
| Digital 25 | Encoder 4B | Digital | Analog 2 | SW10 | Analog In |
| Digital 26 | Encoder 5B | Digital | Analog 3 | SW46 | Analog In |
| Digital 27 | Encoder 5A | Digital | Analog 4 | SW47 | Analog In |
| Digital 28 | Encoder 5A | Digital | Analog 5 | SW48 | Analog In |
| Digital 29 | Enc5 SW | Digital | Analog 6 | SW49 | Analog In |
| Digital 30 | LED1 | Digital | Analog 7 | SW50 | Analog In |
| Digital 54 | SW9 | MCP23017 | Digital 62 | Enc7 SW | MCP23017 |
| Digital 55 | SW1 | MCP23017 | Digital 63 | Enc8 SW | MCP23017 |
| Digital 56 | SW2 | MCP23017 | Digital 64 | SW8 | MCP23017 |
| Digital 57 | SW3 | MCP23017 | Digital 65 | SW7 | MCP23017 |
| Digital 58 | SW4 | MCP23017 | Digital 66 | SW21 | MCP23017 |
| Digital 59 | SW5 | MCP23017 | Digital 67 | SW19 | MCP23017 |
| Digital 60 | SW6 | MCP23017 | Digital 68 | SW20 | MCP23017 |
| Digital 61 | Enc6 SW | MCP23017 | Digital 69 | SW22 | MCP23017 |

14 mechanical Encoders:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Kjell number** | **A function** | **B function** | **s/w number** | **Enc A pin** | **Enc B pin** |
| 2 | RX1 AF gain | RX1 RF gain | 0, 1 | DIG4, DIG5 | DIG7, DIG8 |
| 3 | Filter High cut | Filter Low cut | 2, 3 | DIG10, DIG11 | DIG14, DIG15 |
| 4 | Diversity gain | Diversity phase | 4, 5 | DIG17, DIG22 | DIG24, DIG25 |
| 5 | Mic Gain | Drive | 6, 7 | DIG27, DIG28 | DIG16, DIG26 |
| 6 | RX2 AF gain | RX2 RF gain | 8, 9 | DIG46, DIG47 | DIG12, DIG39 |
| 7 | Comp | Master AF gain | 10, 11 | DIG48, DIG49 | DIG18, DIG19 |
| 8 | Squelch | n/a | 12, 13 | DIG50, DIG51 | DIG35, DIG36 |

34 s/w connected pushbuttons:

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Kjell SW number** | **s/w** | **Function** | **pin** | **Kjell SW number** | **s/w** | **Function** | **pin** |
| SW1 | 19 | A/B toggle | DIG55 | SW19 | 31 | SINGLE CAL | DIG67 |
| SW2 | 20 | MOX | DIG56 | SW20 | 32 | 2 TONE TEST | DIG68 |
| SW3 | 21 | TUNE | DIG57 | SW21 | 30 | PURESIGNAL ON | DIG66 |
| SW4 | 22 | Click TUNE | DIG58 | SW22 | 33 | SNB | DIG69 |
| SW5 | 23 | VFO LOCK | DIG59 | SW46 | 1 | No function (menu 1) | ANA3 |
| SW6 | 24 | A > B | DIG60 | SW47 | 2 | No function (menu 2) | ANA4 |
| SW7 | 29 | B > A | DIG65 | SW48 | 3 | No function (menu 3) | ANA5 |
| SW8 | 28 | SPLIT | DIG64 | SW49 | 4 | No function (menu 4) | ANA6 |
| SW9 | 18 | RIT ON | DIG54 | SW50 | 5 | No function (menu 5) | ANA7 |
| SW10 | 0 | RIT - | ANA2 | ENC2 SW | 6 | RX1 MUTE | DIG6 |
| SW11 | 10 | RIT + | DIG40 | ENC3 SW | 17 | FILTER RESET | DIG53 |
| SW12 | 11 | BAND - | DIG41 | ENC4 SW | 8 | DIVERSITY FINE/COARSE | DIG23 |
| SW13 | 12 | MODE - | DIG42 | ENC5 SW | 9 | No function | DIG29 |
| SW14 | 13 | SDR ON | DIG43 | ENC6 SW | 25 | RX2 MUTE | DIG61 |
| SW15 | 14 | BAND + | DIG44 | ENC7 SW | 26 | COMP ON/OFF | DIG62 |
| SW16 | 15 | MODE + | DIG45 | ENC8 SW | 27 | SQL ON/OFF | DIG63 |
| SW17 | 7 | NR | DIG9 |  |  |  |  |
| SW18 | 16 | NB | DIG52 | SW23 |  | Power (not via Arduino) | N/A |

9 s/w connected LEDs:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Kjell LED number** | **s/w number** | **Function** | **Pin** | **Comment** |
| LED1 | 5 | COMP on | DIG30 | By encoder 7 |
| LED2 | 6 | SQL on | ANA0 | By encoder 8 |
| LED3 | 2 | MOX | ANA1 |  |
| LED4 | 3 | TUNE on | DIG32 |  |
| LED5 | 4 | CTUNE on | DIG33 |  |
| LED6 | 0 | LOCK on | DIG34 |  |
| LED7 | 1 | PS on | DIG37 |  |
| LED8 | 7 | RIT on | DIG38 |  |
| LED9 |  | Power | n/a | Powered directly by Vdd |
| LED10 | 8 | TUNE on | DIG31 | ATU ready for Andromeda |

# THETIS Software Changes

THETIS will need to be edited to accommodate this style of control interface.

1. A serial port will need to be allocated (needs code in the setup form)
2. Code needed to establish a serial connection and pass input data to the command handler (do whatever is done for CAT commands)
3. At initialisation, query the software version in the front panel Arduino
4. Incoming pushbutton and encoder messages to be handled with a “command dispatcher” using a table with the assigned functions for each
5. Changes to settings to update LED indicators again using a table of indicator assignments
6. For pushbuttons: the “dispatcher” for menu buttons can be used
7. For indicators: the logic to highlight menu buttons can be used, probably
8. For encoders, a new dispatcher function is needed. This also needs to handle encoder presses for multifunction encoder and possibly to set one of two functions for a dual encoder.

## Available functions for Each Control

### Indicators and Pushbuttons

For pushbuttons and indicators: try to use the same command set as for the menu buttons. See if any of the following are not available as menu buttons, and add them if needed.

|  |  |
| --- | --- |
| Pushbuttons (including encoder “press”)   * A/B VFO select * MOX * TUNE * AF MUTE (explicit RX1/2 needed) * Filter reset * Band + * Band – * Mode + * Mode – * AGC speed * NB step * NR step * SNB on/off * ANF on/off * Off /RIT on / XIT on * RIT + * RIT – * A>B * B>A * A/B swap * Split * CTUNE * Lock * Radio Start/Stop * Squelch on/off * Attenuation Step * VOX on/off * Diversity fast/slow step * Compander on/off * Puresignal on/off * Puresignal two tones test * Puresignal single cal (deprecated) * MON on / off * Diversity Enable * VFO Sync * Clear RIT/XIT * Filter + * Filter – * VAC1 on/off * VAC2 on/off * Display Centre * F1-F8 button | Indicators   * MOX * TUNE * ATU Ready * RIT on * Split selected * CTune selected * Lock selected * NB off/on * NR off/on * SNB off/on * ANF off/on * Squelch on/off * VFO A/B * Compander on/off * Puresignal on/off * LED lit if encoder 2nd function selected * VFO sync * XIT   Go through and check if these available! |

### Encoders

* RX1 AF gain
* RX2 AF gain
* Sub RX AF Gain
* Master AF gain
* RX1 stereo balance
* RX2 stereo balance
* Sub RX stereo balance
* RX1 AGC
* RX2 AGC
* RX1 step attenuation
* RX2 step attenuation
* RX1 Squelch
* RX2 Squelch
* Selected RX Filter high cut
* Selected RX Filter low cut
* TX Drive
* TX Mic Gain
* VFO A tune
* VFO B tune
* RIT
* VOX gain
* VOX delay
* Compander threshold
* CW sidetone
* CW speed
* Diversity Gain
* Diversity Phase
* Multifunction
* Display Pan
* Display Zoom